10-METER BAND PLAN 
The following chart gives the latest information on the "gentlemen's agreement" that ARRL members follow when using the 10-meter band. 
Frequency Operating Mode Note 
28.000 - 28.070 CW 
28.070 - 28.150 RTTY 
28.150 - 28.190 CW 
28.100 - 28.200 CW New Beacon Band* 
28.200 - 28.300 CW Old Beacon Band* Until 1990
 28.300 - 29.300 Phone
 29.300 - 29.510 Satellites
 29.510 - 29.590 Repeater inputs 
29.600 FM simplex calling frequency 
29.610 - 29.700 Repeater inputs 
*Beacon bands are reserved for special stations. Do not transmit in these bands.